Macros | Functions
ref_app_parking_main.c File Reference
`#include <stdbool.h>`
`#include <stdio.h>`
`#include <stdlib.h>`
`#include "acc_hal_definitions_a121.h"`
`#include "acc_hal_integration_a121.h"`
`#include "acc_integration.h"`
`#include "acc_rss_a121.h"`
`#include "acc_version.h"`
`#include "ref_app_parking.h"`

Go to the source code of this file.

## Macros
#define | SENSOR_ID (1U)

## Functions
int | acconeer_main (int argc, char *argv[])
| Assembly test example. More...

## Macro Definition Documentation

## ◆ SENSOR_ID

#define SENSOR_ID (1U)

Definition at line 18 of file ref_app_parking_main.c.

## Function Documentation

## ◆ acconeer_main()

int acconeer_main | ( | int | argc,
|  | char * | argv[]
| ) |  |

Assembly test example.

Touchless button application.

Tank level reference application.

Smart presence reference application.

Parking application.

Breathing example application.

Waste level application.

Vibration example.

Surface velocity example application.

Service subsweeps example.

Service multple configurations example.

Low power service example.

Service sensor calibration caching example.

Service example.

Processing subtract adaptive background example.

Processing static presence example.

Processing peak interpolation example.

Processing noncoherent mean example.

Processing coherent mean example.

Processing amplitude example.

hand motion application

Detector presence example with multiple configurations.

Low power detector presence example.

Detector presence example.

Detector distance example with iq data print.

Distance detector low power example.

Detector distance with calibration caching example.

Detector distance example.

Control helper example.

Cargo application.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Detector filters and states are reset on prepare (reconfiguration) to avoid risk of false detections when switching back to a zone.

Vibration example configuration

Definition at line 22 of file ref_app_parking_main.c.