Functions
acc_exploration_server_stm32.h File Reference
`#include "acc_exploration_server_base.h"`

Go to the source code of this file.

## Functions
void | acc_exploration_server_stm32_init (const char *hw, char *buffer, size_t buffer_size)
| Init the stm32 exploration server. More...
void | acc_exploration_server_stm32_main (void)
| Start the stm32 exploration server. More...

## Function Documentation

## ◆ acc_exploration_server_stm32_init()

void acc_exploration_server_stm32_init | ( | const char * | hw,
|  | char * | buffer,
|  | size_t | buffer_size
| ) |  |

Init the stm32 exploration server.

Parameters

  [in] | hw | The name of the hardware platform
  [in] | buffer | The buffer used for receiving commands from the client
  [in] | buffer_size | The size of the command buffer

Definition at line 132 of file acc_exploration_server_stm32.c.

## ◆ acc_exploration_server_stm32_main()

void acc_exploration_server_stm32_main | ( | void |  | ) |

Start the stm32 exploration server.

The embedded exploration server for STM32 can stream UART input data directly into the input buffer.

Setup DMA into buffer with buffer_size.

Definition at line 140 of file acc_exploration_server_stm32.c.