### - g -

- get_angle_correction() : example_surface_velocity.c
- get_command() : i2c_distance_detector.c , i2c_presence_detector.c , i2c_ref_app_breathing.c , i2c_example_cargo.c
- get_data_padded_f32_complex() : acc_algorithm.c
- get_data_padded_f32_to_f32_complex() : acc_algorithm.c
- get_detection() : ref_app_touchless_button.c
- get_detector_end_m() : ref_app_tank_level.c
- get_detector_start_m() : ref_app_tank_level.c
- get_gpio_port_clock() : acc_integration_stm32.c
- get_i2c_address() : i2c_application_system_stm32.c
- get_max_buffer_size() : ref_app_smart_presence.c
- get_max_num_points() : ref_app_smart_presence.c
- get_max_num_zones() : ref_app_smart_presence.c
- get_measure_timeout_ms() : ref_app_parking.c
- get_next_empty_cache_index() : example_detector_distance_calibration_caching.c , example_service_calibration_caching.c
- get_peak_distance() : distance_reg_protocol_access.c
- get_peak_strength() : distance_reg_protocol_access.c
- get_perceived_wavelength() : example_surface_velocity.c
- get_pin_state() : i2c_application_system_stm32.c
- get_profile() : acc_algorithm.c
- get_protocol_error_flags() : ref_app_breathing_reg_protocol_access.c , presence_reg_protocol_access.c , distance_reg_protocol_access.c , example_cargo_reg_protocol_access.c
- get_register_struct() : acc_reg_protocol.c
- get_rtc_tick() : acc_integration_stm32.c , i2c_application_system_stm32.c
- get_threshold() : ref_app_touchless_button.c
- get_tick() : acc_exploration_server_stm32.c
- get_velocity_estimate() : example_surface_velocity.c
- get_zero_mean_time_series() : example_vibration.c
- gpio_resume() : acc_integration_stm32.c
- gpio_suspend() : acc_integration_stm32.c