Functions
acc_config_subsweep.h File Reference
`#include <stdint.h>`
`#include "acc_config.h"`
`#include "acc_definitions_a121.h"`

Go to the source code of this file.

## Functions
void | acc_config_num_subsweeps_set (acc_config_t *config, uint8_t num_subsweeps)
| Set the number of subsweeps to use. More...
uint8_t | acc_config_num_subsweeps_get (const acc_config_t *config)
| Get the number of subsweeps to use. More...
void | acc_config_subsweep_start_point_set (acc_config_t *config, int32_t start_point, uint8_t index)
| Set the starting point of the sweep. More...
int32_t | acc_config_subsweep_start_point_get (const acc_config_t *config, uint8_t index)
| Get the starting point of the sweep. More...
void | acc_config_subsweep_num_points_set (acc_config_t *config, uint16_t num_points, uint8_t index)
| Set the number of data points to measure. More...
uint16_t | acc_config_subsweep_num_points_get (const acc_config_t *config, uint8_t index)
| Get the number of data points to measure. More...
void | acc_config_subsweep_step_length_set (acc_config_t *config, uint16_t step_length, uint8_t index)
| Set the step length in a sweep. More...
uint16_t | acc_config_subsweep_step_length_get (const acc_config_t *config, uint8_t index)
| Get the step length in a sweep. More...
void | acc_config_subsweep_profile_set (acc_config_t *config, acc_config_profile_t profile, uint8_t index)
| Set a profile. More...
acc_config_profile_t | acc_config_subsweep_profile_get (const acc_config_t *config, uint8_t index)
| Get the currently used profile. More...
void | acc_config_subsweep_hwaas_set (acc_config_t *config, uint16_t hwaas, uint8_t index)
| Set the hardware accelerated average samples (HWAAS) More...
uint16_t | acc_config_subsweep_hwaas_get (const acc_config_t *config, uint8_t index)
| Get the hardware accelerated average samples (HWAAS) More...
void | acc_config_subsweep_receiver_gain_set (acc_config_t *config, uint8_t gain, uint8_t index)
| Set receiver gain setting. More...
uint8_t | acc_config_subsweep_receiver_gain_get (const acc_config_t *config, uint8_t index)
| Get receiver gain setting. More...
void | acc_config_subsweep_enable_tx_set (acc_config_t *config, bool enable, uint8_t index)
| Enable or disable the transmitter. More...
bool | acc_config_subsweep_enable_tx_get (const acc_config_t *config, uint8_t index)
| Get transmitter enable mode. More...
void | acc_config_subsweep_prf_set (acc_config_t *config, acc_config_prf_t prf, uint8_t index)
| Set Pulse Repetition Frequency. More...
acc_config_prf_t | acc_config_subsweep_prf_get (const acc_config_t *config, uint8_t index)
| Get Pulse Repetition Frequency. More...
void | acc_config_subsweep_phase_enhancement_set (acc_config_t *config, bool enable, uint8_t index)
| Set the phase enhancement enabled configuration. More...
bool | acc_config_subsweep_phase_enhancement_get (const acc_config_t *config, uint8_t index)
| Get the phase enhancement enabled configuration. More...
void | acc_config_subsweep_iq_imbalance_compensation_set (acc_config_t *config, bool enable, uint8_t index)
| Enable or disable the IQ imbalance compensation. More...
bool | acc_config_subsweep_iq_imbalance_compensation_get (const acc_config_t *config, uint8_t index)
| Get the IQ imbalance compensation configuration. More...
void | acc_config_subsweep_enable_loopback_set (acc_config_t *config, bool enable, uint8_t index)
| Set the loopback enabled configuration. More...
bool | acc_config_subsweep_enable_loopback_get (const acc_config_t *config, uint8_t index)
| Get the enable loopback configuration. More...