;PlatformIO User notes:

;It is possible to load settings from the calling program rather than modifying
;the library for each project by modifying the "platformio.ini" file.

;The User_Setup_Select.h file will not load the user setting header files if
;USER_SETUP_LOADED is defined.

;Instead of using #define, use the -D prefix, for example:

; PlatformIO Project Configuration File
;
;   Build options: build flags, source filter, extra scripting
;   Upload options: custom port, speed and extra flags
;   Library options: dependencies, extra library storages
;
; Please visit documentation for the other options and examples
; http://docs.platformio.org/page/projectconf.html

[env:pico]
platform = https://github.com/maxgerhardt/platform-raspberrypi.git
board = pico
framework = arduino
board_build.core = earlephilhower
board_build.filesystem_size = 0.5m
lib_deps = bodmer/TFT_eSPI@^2.5.21
; change microcontroller
board_build.mcu = rp2040

; change MCU frequency
board_build.f_cpu = 133000000L

build_flags =
  -Os
  -DUSER_SETUP_LOADED=1
  ; Define the TFT driver, pins etc here:
  -DTFT_PARALLEL_8_BIT=1
  -DRM68120_DRIVER=1
  -DRP2040_PIO_CLK_DIV=1
  -DTFT_DC=28
  -DTFT_WR=22
  -DTFT_RST=2

  -DTFT_D0=6
  -DTFT_D1=7
  -DTFT_D2=8
  -DTFT_D3=9
  -DTFT_D4=10
  -DTFT_D5=11
  -DTFT_D6=12
  -DTFT_D7=13

  -DTFT_BL=16
  -DTFT_BACKLIGHT_ON=HIGH

  -DLOAD_GLCD=1
  -DLOAD_FONT2=1
  -DLOAD_FONT4=1
  -DLOAD_FONT6=1
  -DLOAD_FONT7=1
  -DLOAD_FONT8=1
  -DLOAD_GFXFF=1
  -DSMOOTH_FONT=1
