Arduino

Reference Language | Libraries | Comparison | Changes

### Extended SPI library usage with the Due

On the Arduino Due, the SAM3X has advanced SPI capabilities. It is possible to use these extended methods, or the AVR-based ones.

The extended API can use pins 4, 10, and 52 for CS.

#### Use

You must specify each pin you wish to use as CS for the SPI devices.

It is possible for the Due to automatically handle the chip selection between multiple devices sharing the SPI bus. Each device may have also different attribues such as speed and datamode.

If using multiple devices with different CS pins, you'll need to declare those pins in setup(). In the following example, there are two devices that share the SPI MISO, MOSI, and SCK pins. One device CS is attached to pin 4, the other to pin 10.

void setup(){
// initialize the bus for a device on pin 4
SPI.begin(4);
// initialize the bus for a device on pin 10
SPI.begin(10);
}
[Get Code]

Once a pin has been declared as a CS pin, it's possible to change its default behaviors as well. For example, if the devices run at different clock speeds, the setup() may look like this :

void setup(){
// initialize the bus for the device on pin 4
SPI.begin(4);
// Set clock divider on pin 4 to 21
SPI.setClockDivider(4, 21);
// initialize the bus for the device on pin 10
SPI.begin(10);
// Set clock divider on pin 10 to 84
SPI.setClockDivider(10, 84);
}
[Get Code]

A single byte transfer to a device on pin 4 could look like this :

void loop(){
byte response = SPI.transfer(4, 0xFF);
}
[Get Code]
In the above, “0xFF” is sent to the SPI device on pin 4 and the data coming from MISO is saved inside the variable response. The chip selection is handled automatically by the SPI controller, the transfer command implies the following:

- Select device by setting pin 4 to LOW
- Send 0xFF through the SPI bus and return the byte received
- Deselect device by setting pin 4 to HIGH

It's possible to send more than one byte in a transaction by telling the the transfer command to not deselect the SPI device after the transfer :

void loop(){
//transfer 0x0F to the device on pin 10, keep the chip selected
SPI.transfer(10, 0xF0, SPI_CONTINUE);
//transfer 0x00 to the device on pin 10, keep the chip selected
SPI.transfer(10, 0×00, SPI_CONTINUE);
//transfer 0x00 to the device on pin 10, store byte received in response1, keep the chip selected
byte response1 = SPI.transfer(10, 0×00, SPI_CONTINUE);
//transfer 0x00 to the device on pin 10, store byte received in response2, deselect the chip
byte response2 = SPI.transfer(10, 0×00);
}
[Get Code]
The parameter SPI_CONTINUE ensures that chip selection is keep active between transfers. On the last transfer SPI_CONTINUE is not specified as it's the last byte transferred.

See the individual reference pages for setClockDivider(), setDataMode(), transfer(), setBitOrder() for proper syntax when using the extended methods.

NB : once SPI.begin() is called, the declared pin will not be available as a general purpose I/O pin
Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- Careers