Arduino

Reference Language | Libraries | Comparison | Changes

Servo

## writeMicroseconds()

#### Description

Writes a value in microseconds (uS) to the servo, controlling the shaft accordingly. On a standard servo, this will set the angle of the shaft. On standard servos a parameter value of 1000 is fully counter-clockwise, 2000 is fully clockwise, and 1500 is in the middle.

Note that some manufactures do not follow this standard very closely so that servos often respond to values between 700 and 2300. Feel free to increase these endpoints until the servo no longer continues to increase its range. Note however that attempting to drive a servo past its endpoints (often indicated by a growling sound) is a high-current state, and should be avoided.

Continuous-rotation servos will respond to the writeMicrosecond function in an analogous manner to the write function.

#### Syntax

servo.writeMicroseconds(uS)

#### Parameters

servo: a variable of type Servo

uS: the value of the parameter in microseconds (int)

#### Example

    #include <Servo.h>

    Servo myservo;

    void setup()
    {
      myservo.attach(9);
      myservo.writeMicroseconds(1500);  // set servo to mid-point
    }

    void loop() {}

#### See also

- attach()
- read()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- Careers