Arduino

Reference Language | Libraries | Comparison | Changes

## char

#### Description

A data type that takes up 1 byte of memory that stores a character value. Character literals are written in single quotes, like this: 'A' (for multiple characters - strings - use double quotes: "ABC").

Characters are stored as numbers however. You can see the specific encoding in the ASCII chart. This means that it is possible to do arithmetic on characters, in which the ASCII value of the character is used (e.g. 'A' + 1 has the value 66, since the ASCII value of the capital letter A is 65). See Serial.println reference for more on how characters are translated to numbers.

The char datatype is a signed type, meaning that it encodes numbers from -128 to 127. For an unsigned, one-byte (8 bit) data type, use the byte data type.

#### Example

      char myChar = 'A';
      char myChar = 65;      // both are equivalent

#### See also

- byte
- int
- array
- Serial.println

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- Careers