Arduino

Reference Language | Libraries | Comparison | Changes

GSM : GSMClient class

## write()

#### Description

Write data to the server the client is connected to.

#### Syntax

client.write(data)
client.write(buffer)
client.write(buffer, size)

#### Parameters

- data: the value to write (byte or char)
- buffer : an array of data (byte or char) to write
- size : size of the buffer to write (byte)

#### Returns

byte - write() returns the number of bytes written. It is not necessary to read this.

#### See Also

- ready()
- connect()
- beginWrite()
- write()
- endWrite()
- connected()
- read()
- available()
- peek()
- flush()
- stop()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- Careers