Arduino

Reference Language | Libraries | Comparison | Changes

## unsigned long

#### Description

Unsigned long variables are extended size variables for number storage, and store 32 bits (4 bytes). Unlike standard longs unsigned longs won't store negative numbers, making their range from 0 to 4,294,967,295 (2^32 - 1).

#### Example

    unsigned long time;

    void setup()
    {
      Serial.begin(9600);
    }

    void loop()
    {
      Serial.print("Time: ");
      time = millis();
      //prints time since program started
      Serial.println(time);
      // wait a second so as not to send massive amounts of data
      delay(1000);
    }

#### Syntax

        unsigned long var = val;

- var - your long variable name
- val - the value you assign to that variable

#### See Also

- byte
- int
- unsigned int
- long
- Variable Declaration

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- Careers