What:		/sys/devices/platform/_UDC_/gadget/suspended
Date:		April 2010
Contact:	Fabien Chouteau <fabien.chouteau@barco.com>
Description:
		Show the suspend state of an USB composite gadget.
		1 -> suspended
		0 -> resumed

		(_UDC_ is the name of the USB Device Controller driver)

What:           /sys/devices/platform/_UDC_/gadget/gadget-lunX/nofua
Date:           July 2010
Contact:        Andy Shevchenko <andy.shevchenko@gmail.com>
Description:
		Show or set the reaction on the FUA (Force Unit Access) bit in
		the SCSI WRITE(10,12) commands when a gadget in USB Mass
		Storage mode.

		Possible values are:
			1 -> ignore the FUA flag
			0 -> obey the FUA flag
