Kernel driver w83795
====================

Supported chips:
  * Winbond/Nuvoton W83795G
    Prefix: 'w83795g'
    Addresses scanned: I2C 0x2c - 0x2f
    Datasheet: Available for download on nuvoton.com
  * Winbond/Nuvoton W83795ADG
    Prefix: 'w83795adg'
    Addresses scanned: I2C 0x2c - 0x2f
    Datasheet: Available for download on nuvoton.com

Authors:
    Wei Song (Nuvoton)
    Jean Delvare <khali@linux-fr.org>


Pin mapping
-----------

Here is a summary of the pin mapping for the W83795G and W83795ADG.
This can be useful to convert data provided by board manufacturers
into working libsensors configuration statements.

    W83795G			|
  Pin	| Name			| Register	| Sysfs attribute
------------------------------------------------------------------
   13	| VSEN1 (VCORE1)	| 10h		| in0
   14	| VSEN2 (VCORE2)	| 11h		| in1
   15	| VSEN3 (VCORE3)	| 12h		| in2
   16	| VSEN4			| 13h		| in3
   17	| VSEN5			| 14h		| in4
   18	| VSEN6			| 15h		| in5
   19	| VSEN7			| 16h		| in6
   20	| VSEN8			| 17h		| in7
   21	| VSEN9			| 18h		| in8
   22	| VSEN10		| 19h		| in9
   23	| VSEN11		| 1Ah		| in10
   28	| VTT			| 1Bh		| in11
   24	| 3VDD			| 1Ch		| in12
   25	| 3VSB			| 1Dh		| in13
   26	| VBAT			| 1Eh		| in14
    3	| VSEN12/TR5		| 1Fh		| in15/temp5
    4	| VSEN13/TR5		| 20h		| in16/temp6
  5/  6	| VDSEN14/TR1/TD1	| 21h		| in17/temp1
  7/  8	| VDSEN15/TR2/TD2	| 22h		| in18/temp2
  9/ 10	| VDSEN16/TR3/TD3	| 23h		| in19/temp3
 11/ 12	| VDSEN17/TR4/TD4	| 24h		| in20/temp4
   40	| FANIN1		| 2Eh		| fan1
   42	| FANIN2		| 2Fh		| fan2
   44	| FANIN3		| 30h		| fan3
   46	| FANIN4		| 31h		| fan4
   48	| FANIN5		| 32h		| fan5
   50	| FANIN6		| 33h		| fan6
   52	| FANIN7		| 34h		| fan7
   54	| FANIN8		| 35h		| fan8
   57	| FANIN9		| 36h		| fan9
   58	| FANIN10		| 37h		| fan10
   59	| FANIN11		| 38h		| fan11
   60	| FANIN12		| 39h		| fan12
   31	| FANIN13		| 3Ah		| fan13
   35	| FANIN14		| 3Bh		| fan14
   41	| FANCTL1		| 10h (bank 2)	| pwm1
   43	| FANCTL2		| 11h (bank 2)	| pwm2
   45	| FANCTL3		| 12h (bank 2)	| pwm3
   47	| FANCTL4		| 13h (bank 2)	| pwm4
   49	| FANCTL5		| 14h (bank 2)	| pwm5
   51	| FANCTL6		| 15h (bank 2)	| pwm6
   53	| FANCTL7		| 16h (bank 2)	| pwm7
   55	| FANCTL8		| 17h (bank 2)	| pwm8
 29/ 30	| PECI/TSI (DTS1)	| 26h		| temp7
 29/ 30	| PECI/TSI (DTS2)	| 27h		| temp8
 29/ 30	| PECI/TSI (DTS3)	| 28h		| temp9
 29/ 30	| PECI/TSI (DTS4)	| 29h		| temp10
 29/ 30	| PECI/TSI (DTS5)	| 2Ah		| temp11
 29/ 30	| PECI/TSI (DTS6)	| 2Bh		| temp12
 29/ 30	| PECI/TSI (DTS7)	| 2Ch		| temp13
 29/ 30	| PECI/TSI (DTS8)	| 2Dh		| temp14
   27	| CASEOPEN#		| 46h		| intrusion0

    W83795ADG			|
  Pin	| Name			| Register	| Sysfs attribute
------------------------------------------------------------------
   10	| VSEN1 (VCORE1)	| 10h		| in0
   11	| VSEN2 (VCORE2)	| 11h		| in1
   12	| VSEN3 (VCORE3)	| 12h		| in2
   13	| VSEN4			| 13h		| in3
   14	| VSEN5			| 14h		| in4
   15	| VSEN6			| 15h		| in5
   16	| VSEN7			| 16h		| in6
   17	| VSEN8			| 17h		| in7
   22	| VTT			| 1Bh		| in11
   18	| 3VDD			| 1Ch		| in12
   19	| 3VSB			| 1Dh		| in13
   20	| VBAT			| 1Eh		| in14
   48	| VSEN12/TR5		| 1Fh		| in15/temp5
    1	| VSEN13/TR5		| 20h		| in16/temp6
  2/  3	| VDSEN14/TR1/TD1	| 21h		| in17/temp1
  4/  5	| VDSEN15/TR2/TD2	| 22h		| in18/temp2
  6/  7	| VDSEN16/TR3/TD3	| 23h		| in19/temp3
  8/  9	| VDSEN17/TR4/TD4	| 24h		| in20/temp4
   32	| FANIN1		| 2Eh		| fan1
   34	| FANIN2		| 2Fh		| fan2
   36	| FANIN3		| 30h		| fan3
   37	| FANIN4		| 31h		| fan4
   38	| FANIN5		| 32h		| fan5
   39	| FANIN6		| 33h		| fan6
   40	| FANIN7		| 34h		| fan7
   41	| FANIN8		| 35h		| fan8
   43	| FANIN9		| 36h		| fan9
   44	| FANIN10		| 37h		| fan10
   45	| FANIN11		| 38h		| fan11
   46	| FANIN12		| 39h		| fan12
   24	| FANIN13		| 3Ah		| fan13
   28	| FANIN14		| 3Bh		| fan14
   33	| FANCTL1		| 10h (bank 2)	| pwm1
   35	| FANCTL2		| 11h (bank 2)	| pwm2
   23	| PECI (DTS1)		| 26h		| temp7
   23	| PECI (DTS2)		| 27h		| temp8
   23	| PECI (DTS3)		| 28h		| temp9
   23	| PECI (DTS4)		| 29h		| temp10
   23	| PECI (DTS5)		| 2Ah		| temp11
   23	| PECI (DTS6)		| 2Bh		| temp12
   23	| PECI (DTS7)		| 2Ch		| temp13
   23	| PECI (DTS8)		| 2Dh		| temp14
   21	| CASEOPEN#		| 46h		| intrusion0
