What:           state
Date:           Sep 2010
KernelVersion:  2.6.37
Contact:        Vernon Mauery <vernux@us.ibm.com>
Description:    The state file allows a means by which to change in and
                out of Premium Real-Time Mode (PRTM), as well as the
                ability to query the current state.
                    0 => PRTM off
                    1 => PRTM enabled
Users:          The ibm-prtm userspace daemon uses this interface.


What:           version
Date:           Sep 2010
KernelVersion:  2.6.37
Contact:        Vernon Mauery <vernux@us.ibm.com>
Description:    The version file provides a means by which to query
                the RTL table version that lives in the Extended
                BIOS Data Area (EBDA).
Users:          The ibm-prtm userspace daemon uses this interface.


