What:		/sys/class/c2port/
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/ directory will contain files and
		directories that will provide a unified interface to
		the C2 port interface.

What:		/sys/class/c2port/c2portX
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/ directory is related to X-th
		C2 port into the system. Each directory will contain files to
		manage and control its C2 port.

What:		/sys/class/c2port/c2portX/access
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/access file enable the access
		to the C2 port from the system. No commands can be sent
		till this entry is set to 0.

What:		/sys/class/c2port/c2portX/dev_id
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/dev_id file show the device ID
		of the connected micro.

What:		/sys/class/c2port/c2portX/flash_access
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/flash_access file enable the
		access to the on-board flash of the connected micro.
		No commands can be sent till this entry is set to 0.

What:		/sys/class/c2port/c2portX/flash_block_size
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/flash_block_size file show
		the on-board flash block size of the connected micro.

What:		/sys/class/c2port/c2portX/flash_blocks_num
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/flash_blocks_num file show
		the on-board flash blocks number of the connected micro.

What:		/sys/class/c2port/c2portX/flash_data
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/flash_data file export
		the content of the on-board flash of the connected micro.

What:		/sys/class/c2port/c2portX/flash_erase
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/flash_erase file execute
		the "erase" command on the on-board flash of the connected
		micro.

What:		/sys/class/c2port/c2portX/flash_erase
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/flash_erase file show the
		on-board flash size of the connected micro.

What:		/sys/class/c2port/c2portX/reset
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/reset file execute a "reset"
		command on the connected micro.

What:		/sys/class/c2port/c2portX/rev_id
Date:		October 2008
Contact:	Rodolfo Giometti <giometti@linux.it>
Description:
		The /sys/class/c2port/c2portX/rev_id file show the revision ID
		of the connected micro.
